**Nuts and Bolts of Deploying Real Cloudproxy Applications**

John Manferdelli[[1]](#footnote-1), Sidarth Telang

**Overview**

Cloudproxy is a software system that provides *authenticated* isolation, confidentiality and integrity of program code and data for programs even when these programs run on remote computers operated by powerful, and potentially malicious system administrators. Cloudproxy defends against observation or modification of program keys, program code and program data by persons (including system administrators), other programs or networking infrastructure. In the case of the cloud computing model, we would describe this as protection from co-tenants and data center insiders. To achieve this, Cloudproxy uses two components: a “Host System” (raw hardware, Virtual Machine Manager, Operating System) which provides capabilities described below to the protected program or “Hosted System” (VM, Application, Container).

This document focuses on installation, security and deployment tradeoffs for Cloudproxy applications. In addition, we explain at length several options for providing key management and program operation continuity as programs are upgraded or new programs are introduced. Programmers new to Cloudproxy often worry that program upgrade is impossible or difficult but it is not. We also describe successful key management strategies which support frequent key rotation which is strongly recommended to ensure ongoing security as standard practice as well as providing resilience in the face of errors or omissions.

We hope these instructions allow safe and rapid installation and configuration of Cloudproxy nodes without extensive training or preparation. We assume readers are familiar with [4] which explains Cloudproxy basic concept like measurement and principal names and explains how to build Cloudproxy applications.

Readers can consult [1] for a fuller description. Source code for Cloudproxy as well as all the samples and documentation referenced here is in [2].

**Downloading and compiling Cloudproxy**

First, you should download the Cloudproxy repository from [2]. To do this, assuming you have git repository support, type

git clone <https://github.com/jlmucb/cloudproxy>,

or,

go get <https://github.com/jlmucb/cloudproxy>.

This latter command will also install the needed go libraries. You can also download a zipped repository from github. You should probably install this in ~/src/github.com/jlmucb (which we refer to as $CLOUDPROXYDIR) to save go compilation problems later. It’s a good idea to put go binaries in ~/bin as is common in Go. Follow the installation instructions in $CLOUDPROXYDIR/Doc; that directory also contains [1] and an up to date version of [4].

You must also install the Go development tools (and C++ development tools if you use the C++ version) as well as protobuf, gtest and gflags as described in the Go documentation.

We will continue to use the simpleexample application described in [4].

**Security Model**

Any deployment of a security system must consider the security or threat model that a system seeks to provide. For the purpose of this Deployment Guide, we consider you are running software for your clients in a cloud data center (or other shared facility) and storing your data there.

Your goal is to provide the principled, verifiable *confidentiality and integrity* of the execution of your programs and the data they read and store from unrestricted attacks from outsiders (e.g. – other clients of the cloud provider) as well as attacks from individual insiders in the cloud data center.

We do assume that data center insiders do not have physical access to computers running your software while that software is running. If they did, insiders could mount physical attacks on running hardware, for example, attaching memory probes to buses. This level of protection can be ensured by, say, enclosing the computers running client software in locked cages that prevent physical access to designated computers while the computers are running Cloudproxy, and for a few minutes afterwards (to protect against insiders harvesting memory remnants of running programs). An extra measure to ensure compliance might be cameras monitoring the caged systems. We *do not* require all computers or networking equipment to be in such cages. In fact, storage systems and networking equipment could remain unprotected without violating the foregoing security guarantee.

We also require that the software you provide (or use) not have remotely exploitable vulnerabilities but we *do not* limit what software you can run or significantly change the common programming model.

**Overview of installation on Linux**

The figure below should be familiar from [4]. We will refer to this throughout the document.

![](data:application/pdf;base64,)

![](data:application/pdf;base64,)

All the hardware enforced mechanisms described in this document are based on the primary system software being Linux based. This includes a native Linux booted on an Intel SMX/TPM platform as well as the KVM hypervisor. Two configurations we discuss (a hosted Linux stacked on KVM and a Docker based Tao stacked on a Linux Tao) do not run directly on hardware but are hosted by a lower level Linux based Tao. We refer to a Cloudproxy Host booted on hardware as a Base CloudProxy Host. The comments in this section thus refer to a KVM base system or a native Linux Base CloudProxy system. With fairly minor changes, one could also make an BSD based platform a Base CloudProxy Host.

The need to perform a measured requires a little more software support. Linux Base CloudProxy Host use a multi-boot sequence to load the Linux kernel mediated by Grub. The stack of booting software consists of:

1. Grub which loads the other booting software into memory.
2. Tboot which mediates the authenticated boot using SMX and the TPM.
3. The Linux kernel with TPM support.
4. A custom initramfs which is measured as part of the boot and contains the compiled Cloudproxy components and critical libraries. Unlike the normal boot sequence, the initram filesystem remains the root file system throughout the base system’s activation. All other file systems are mounted under it. Note that all such mounted file systems (as well and any network connected storage) are treated as untrusted by Cloudproxy programs, and files are encrypted and integrity protected for reading and writing.
5. Dmcrypt which is used to encrypt the page-file and swap space[[2]](#footnote-2) (so no unencrypted data is stored on the paging disk).

We describe the role and general installation procedure for each of these below. For each, there is also an appendix with detailed installation instructions. In addition, we describe preparing, measuring and running Linux based VM’s with Cloudproxy support which can be hosted by KVM.

The overall procedure for preparing and installing Cloudproxy root system is:

1. Install Linux. TPM2.0 requires a Version 4 kernel or later. The kernel should contain the appropriate tpm driver and dmcrypt. We remark that, for security reasons, the TCB of the root CloudProxy system should be as small as possible. A carefully constrained kernel is a critical element of security. For example, our Linux root CloudProxy systems either disallow loading dynamic modules or subject proposed loads to a small whitelist of signed modules. The root CloudProxy should include Dmcrypt.
2. Install the Linux Kernel Development environment, on development machines.
3. Enable SMX, IOMMU and VT extensions in BIOS. Activate the TPM using the BIOS in the case of TPM 2.0 or using trousers in the case of TPM 1.2.
4. Take ownership of the TPM and generate the appropriate keys.
5. Build TBOOT. Retrieve the required Authenticated Code Module (ACM) required by Tboot and place it and the tboot image in /boot as described below.
6. Build the Cloudproxy binaries. Then build a custom initramfs with these binaries as described below. Put the newly created initramfs in /boot/
7. Configure Grub. You will boot a grub configuration which names Tboot, the ACM, your Linux kernel and your custom Initramfs.
8. Boot!

The “measurement” of a TPM mediated boot will be in PCR 17 and 18 of your TPM. You will need this measurement for your domain service and the easiest way to get it is to have Cloudproxy report it after it boots on your test hardware. Cloudproxy does the rest! After you have successfully carried out these steps, you can build applications as described in [4].

Next, we describe each of these steps in more detail. After that, we discuss secure, scalable deployment of Cloudproxy applications including key management techniques followed by a brief description of Security Considerations which should be thought through for your particular deployment needs.

**Hardware root of trust**

Because of a lack of physical control over the hardware (and even with physical control in the face of errors), maintaining our security model requires a hardware root of trust that is used to measure the base system software that boots and ensure that only software and only software trusted by you can access some basic system secrets like signing keys. Without this, insiders could boot any privileged software and violate the security model you seek to enforce. Cloudproxy, as mentioned above can employ TPM1.2 or TPM 2.0 as “off the shelf” mechanisms. So first you must enable and provision one of these.

**BIOS**

In Bios, you must ensure that VT and IOMMU support is enabled. The Tpm must also be enabled (usually it is enabled by default in the case of TPM 2.0 but is disabled by default with TPM 1.2).

## **Trusted Platform Module (TPM**)

The TPM is a dedicated microprocessor designed to offer facilities for generation of cryptographic keys, random number generation, remote attestation and data sealing. In this document, we use the TPM as the hardware root of trust of our Cloudproxy system.

To use the TPM we need to enable it, and take ownership of it. Taking ownership of a TPM is the process of setting up an authorization value (e.g. – a password), which is subsequently required for certain kinds of TPM operations.

Taking ownership of a TPM is the process of setting up authorization values (eg. passwords) for the *ownerAuth*, *endorsementAuth*, and *lockoutAuth* types of authorization. Different TPM commands require different types of authorization. A cleared TPM (using TPM2\_Clear) has these values set to *emptyAuth.*

Here are instructions for TPM 1.2 and TPM 2.0.

**TPM 1.2**

There are several keys in a TPM 1.2, which include:

1. TPM Endorsement Key (EK): This key is created by the manufacturer and cannot be removed. Sometimes it can be changed by the owner of the computer.
2. TPM Storage Root Key (SRK): Is the 2048 bit RSA key created when configuring the ownership. This key is stored inside the chip and can be removed. This key is also used to seal/unseal data.
3. TPM Attestation Identity Key (AIK): This key is used by the TPM to sign attestations (to the state of the PCRs). It is encrypted and integrity protected by the SRK.

Cloudproxy uses the SRK to seal/unseal data and the AIK to sign attestations. However, all we need to get Cloudproxy running is an AIK blob. Following are instructions on how to obtain it, and to provision the TPM for use by Cloudproxy.

1. First, we install tools needed to talk to the TPM device.  
   go get -u -v github.com/google/go-tpm/…
2. Reset your TPM device as follows.  
     
   - Disable the TPM device on your BIOS screen.  
   - Reboot the system **by powering off**, re-enable the TPM device in BIOS, and select the option to clear the device if you see one.  
     
   TPM devices require an assertion of physical presence to be cleared, and for most machines powering off and on does the trick. But ultimately how presence is asserted depends on your machine, so consult your BIOS manual for detailed instructions.  
   Also, note that the TPM device comes disabled by default.
3. Take ownership of the device, which may need root privileges. Note that tpm-takeownership takes the new owner and SRK password from the environment, and that we do not set them. The current Cloudproxy implementation assumes these authorizations are not set, when talking to the TPM.  
   unset TPM\_OWNER\_AUTH  
   unset TPM\_SRK\_AUTH  
   sudo su --preserve-environment  
   tpm-takeownership
4. Generate the aikblob and set permissions so that Cloudproxy may read it (note that this blob is encrypted and integrity protected by the TPM so it can be made public).  
   genaik  
   chmod 777 aikblob

Some troubleshooting tips can be found in the appendix.

**TPM 2.0**

Taking ownership of a TPM 2.0 is the process of setting up authorization values (eg. passwords) for the *ownerAuth*, *endorsementAuth*, and *lockoutAuth* types of authorization. Different TPM 2.0 commands require different types of authorization. A cleared TPM (using TPM2\_Clear) has these values set to *emptyAuth.* To use Cloudproxy, we need to set each of the above authorization to *emptyAuth* (i.e. empty string as a password).

Enabling, taking ownership of and clearing a TPM 2.0 device is done entirely through BIOS. Consult your BIOS manual for detailed steps. Detailed instructions for the Intel NUC 5i5MYHE can be found in the appendix.

**Tboot**

Trusted Boot (tboot) is a pre-kernel/VMM module that uses Intel Trusted Execution Technology (Intel TXT) to perform a measured and verified launch of an OS kernel/VMM. It uses the TPM for this and when successfully run, it stores the kernel/VMM measurement in the TPM PCRs, which is then read by the root CloudProxy Tao.

**Installation overview**: After making sure your TPM device is enabled (see previous sections), download the tboot source tarball from sourceforge.net, and build and install using make and sudo make install. This build a tboot.gz image and places it in /boot for your bootloader to use when booting up. You will also need a SINIT AC module for your type of processor that you must manually place in /boot. This module enables TXT to load tboot. Finally you need to update your bootloader configuration to load tboot. Detailed instructions are in the appendix.

Some miscellaneous but probably useful notes on tboot follow.

**txt-stat**: The txt-stat tool installed by tboot is a Linux application that reads some of the TXT registers and will display the tboot boot log if tboot was run with 'logging=memory'. It is useful to run after a boot-up to check if tboot was run successfully.

**Launch control policy (LCP) and Verified Launch Policy (VLP)**: These are policies that govern which measured launch environments (MLEs, for eg. tboot) and kernels TXT and tboot are allowed to launch respectively. Tboot comes with a set of tools to install LCPs and VLPs, however they are not needed for CloudProxy.

**PCR values after trusted boot**:  
  
PCR 17 :  
 It will be extended with the following values (in this order):  
 - The values as documented in the MLE Developers Manual  
 - SHA-1 hash of: tboot policy control value (4 bytes) |  
 SHA-1 hash of tboot policy (20 bytes)  
 : where the hash of the tboot policy will be 0s if TB\_POLCTL\_EXTEND\_PCR17 is clear  
PCR 18 :  
 It will be extended with the following values (in this order):  
 - SHA-1 hash of tboot (as calculated by lcp\_mlehash)  
 - SHA-1 hash of first module in grub.conf (e.g. Xen or Linux kernel)

Detailed copy and paste instructions are in the appendix.

**Preparing the Linux or KVM image**

**InitRamfs**

Everything upon which the security of your software relies must be measured, including basic system software and libraries you rely on. On Linux, we can protect and measure all that requires protection by incorporating it into a small, in memory, filesystem provided with the kernel boot image.

Initram is an in memory file system used by the Linux kernel. In most cases, initramfs is discarded late in the boot sequence of Linux in favor of the “real” mounted system disk but in our case, initram remains the root file system throughout the Base Linux Cloudproxy lifetime (other file systems are mounted under it). We modify “stock” initramfs in several ways. First, we get rid of any unnecessary functionality. Next we include the Cloudproxy components and, in some cases, even the Cloudproxy applications are included in initramfs. Lastly, we modify the stock scripts so that the “disk based” root file system is mounted under the initramfs rather than replacing it.

Detailed copy and paste instructions for initramfs are in the appendix.

**Dmcrypt**

Since most Linux systems employ virtual memory systems which temporarily store memory pages on disk, we must prevent secrets from being saved to a disk in a way that could be modified as programs are running or read after programs stop running. This would violate our security model. To do this, we employ dmcrypt which encrypts the disk used for paging. We also assume this disk is contained within the cage housing the Cloudproxy programs (since dmcrypt does not provide integrity protection). However, we *do not* require that the paging disk be protected before or after being used.

Detailed copy and paste instructions for configuring Linux to use dmcrypt are in the appendix.

**Grub configuration**

Grub is used to load the ACM, tboot, the OS (or hypervisor) and initramfs into main memory so that the measured boot can be carried out. Note that one can employ a grub configuration that can boot non Cloudproxy enabled images without harm.

This is done automatically by Tboot. Detailed copy and paste instructions for grub setup are in the appendix.

**Installing and configuring a Cloudproxy supported KVM instance**

We use KVM as the Cloudproxy hypervisor that can host isolated, measured Cloudproxy VMs.

Detailed copy and paste instructions for KVM setup are in the appendix.

**Installing and configuring a Cloudproxy supported TPM hosted Linux**

In addition to a hypervisor rooted Cloudproxy stack, one could simply boot a Cloudproxy enabled Linux.

Detailed copy and paste instructions for Linux root setup are in the appendix.

**Installing and configuring a Linux stacked on KVM**

When using a hypervisor rooted Cloudproxy system, we need to provide Cloudproxy enabled VMs. Cloudproxy can support “stacked” systems that extend root protection to any layer of a software stack.

Detailed copy and paste instructions for configuring a stacked Linux Tao are in the appendix.

**Installing and configuring Docker containers**

Another stacked system protected by Cloudproxy is a Docker container within a Linux host (or stacked Linux host).

Detailed copy and paste instructions for configuring and running a stacked Docker Tao are in the appendix.

**Host Certificates**

Your TPM must have a signed certificate for its attest key. The underlying key is called an AIK in the case of TPM 1.2 and an Endorsement Certificate in the case of TPM 2.0. Consult the final appendix to provision this certificate for TPM 1.2 and TPM 2.0. In many cases, an Endorsement Certificate, signed by the manufacturer, is included in NVRam for TPM 2.0.

**Domains**

Domains and domain initialization was covered in [5] but when booting under TPM 1.2 and TPM 2.0, it is important to specify the proper PCR’s and, in the case of TPM 1.2, make sure the AIK was signed by the policy key using XXXX and, in the case of TPM 2.0 roots make sure the attest\_service is running.

**SimpleExample with TPM Tao’s**

Complete instructions on running *simpleexample* under a TPM 1.2 Tao and a TPM 2.0 Tao appear in an appendix**.**

**Considerations in deploying Cloudproxy**

**Key management**

Key management supports the storage, distribution and critically, the rotation of symmetric content keys as well as establishing the “Program Key” for Cloudproxy programs (and hosts) and rotating the Program Key as keys expire or cloudproxy programs are changed.

In most of our programs, keys and content types (like files) are objects and have domain-wide hierarchical universal names and epochs. Epochs are monotonically increased. For example, a file used by several Cloudproxy programs may contains customer information like customer names, addresses, etc. Since these are stored objects, they are encrypted and integrity protected and typically stored redundantly at several network accessible locations. The file /jlm/file/us-zone/customer-file-location1, epoch 2, type: file refers to the file with the indicated name; the epoch indicates the version of the file, different versions of the file are usually encrypted with different keys. These encryption keys also have domain-wide hierarchical universal names and epochs. Encryption keys protect other objects like keys or files. To decrypt a file, we need a chain of keys starting at the sealing key for the Cloudproxy program on a given node and terminating in the desired object (say a file). Each node of the chain consists of the name of the protector object, the protected objects and an encrypted blob consisting of the protected object encrypted (and integrity protected) by the protector key.

For example

/jlm/program-name/master-sealing-key, epoch 5, type: aes-128-gcm

/jlm/key/us-zone/customer-folder-keys, epoch 2, type: aes-128-gcm

/jlm/key/us-zone/customer-file-key, epoch 3, type: aes-128-gcm

/jlm/file/us-zone/customer-file-location1, epoch 2, type: file

Often domains will want to partition keys to provide resilience by *protection zones.* One common way to do this is to have different keys for different geographic locations. This is easily accomplished by reserving a level of the hierarchical object namespace for the zone name as is done above.

Although the foregoing name, epoch based mechanisms facilitate key rotation, it is not a complete solution. Let’s first consider, given this framework, how we might rotate keys.

There are two common circumstances where new keys are introduced into a Cloudproxy environment. First, keys should be rotated regularly as part of good cryptographic hygiene and second, when programs change, their measurements change which means they can no longer access sealed data for earlier versions of the program. In both cases, similar techniques can be used to carry out the key rotation.

**Key Rotation and software upgrades**

See go/support/support\_libraries /protected-objects and go/support/support\_libraries/ rotation\_support for support routines to maintain and encrypt content keys and build chains of keys like:

Protector Object: /jlm/program-name/master-sealing-key, epoch 5, type: aes-128-gcm

Protected Object: /jlm/key/us-zone-key, epoch 2, type: aes-128-gcm

Encrypted Protected Object

Protector Object: /jlm/key/us-zone-key, epoch 2

Protected Object: /jlm/key/us-zone-key/customer-folder-key, epoch 3, type: aes-128-gcm

Encrypted Protected Object

Protector Object: /jlm/key/us-zone-key/ customer-folder-key, epoch 3

Protected Object: /jlm/key/us-zone-key/customer-folder-key/customer-file-key, epoch 2, type: aes-128-gcm

Encrypted Protected Object

Protector Object: /jlm/key/us-zone/customer-file-key, epoch 3, type: aes-128-gcm

Protected Object: /jlm/file/us-zone/customer-file-location1, epoch 2, type: file

*Using a keystore*

A sample keystore with the required functionality is implemented in $CLOUDPROXY/go/support/infrastructure\_support/CPSecretServer. Needless to say, this program itself would likely be implemented as a cloudproxy program.

![](data:application/pdf;base64,)

Since keys can be fetched any time after startup and no pre-existing state is required (except for the Program key), key rotation is easy and is focused at the Secret Service. The secret service can also publish alerts when new keys are available. Upgrade when program versions change is also easy. The new version of the program just gets keys from the server. The server is updated with new ACLs as new program versions become available.

*Using policy key disclosure*

![](data:application/pdf;base64,)

See $CLOUDPROXY/go/support/support\_libraries/secret\_disclosure\_support for sample code to construct and verify a policy-key signed secret-disclosure statement.

Policy-key says PrincipalName can-read /jlm/key/us-zone/customer-folder-key, epoch 2

*A note on key rotation*

Either the keystore mechanism or the secret disclosure mechanism can be used to protect other keys. For example, they can help disclose private signing keys to controlled groups. This allows a program to authenticate itself as a group or a standard Linux “service account,” making interoperability with “legacy” authorization systems easier.

**Scale and deployment considerations**

Redundancy, backup, audit, logging, dashboards, predicting problems, forensics

**Just write your applications properly: simple, right?**

While the Cloudproxy security model makes security reliance transparent and easily manageable, you still have to write your programs so that adversaries cannot exploit flaws in the programs you write (or the author of the VMM or BIOS wrote). This is not a trivial task but more programming tools, better programming languages and new techniques (such as proof-carrying-code) present plausible models for “much safer” software you can trust.

**Oops: What to do if there’s a gigantic breach**

Although it is hopefully a rare event, a large scale failure (maybe caused by flaws in critical software) can be remedied simply by redistributing the application with a new policy key (after fixing the security flaws in this case).

**Planned features**

Local state rollback support, a few more crypto algs

**Out of town, call collect**

Bugs, suggestions

**Acknowledgements**

Tom Roeder, Fred Schneider, Kevin Walsh.

**References**

**[1] Manferdelli, Roeder, Schneider, The CloudProxy Tao for Trusted Computing,** <http://www.eecs.berkeley.edu/Pubs/TechRpts/2013/EECS-2013-135.pdf>.

**[2] CloudProxy Source code,** <http://github.com/jlmucb/cloudproxy>. Kevin Walsh and Tom Roeder were principal authors of the Go version.

**[3] TCG, TPM specs,** <http://www.trustedcomputinggroup.org/resources/tpm_library_specification>

**[4]** **Beekman, Manferdelli, Wagner,** Attestation Transparency: Building secure Internet services for legacy clients**.** AsiaCCS, 2016.

**[5] Manferdelli**, CloudProxy Nuts and Bolts.

**[6] Intel,** The MLE Development Guide

**Appendix 1 - Supported Hardware**

Intel or AMD CPU’s and chipsets with secure extensions that support SKINIT. In addition, there must be a physical TPM on the motherboard or in firmware. Most new Intel CPU’s have firmware TPM’s so most new hardware is “automatically” Cloudproxy enabled.

Dell Omniplex

HP xxx laptops

Tom’s laptop

NUC (be sure it supports SMX)

**TPM 1.2 Initialization and Operation (Optional)**

Trousers supports some TPM initialization operations but we have tried to structure installation so that you do not need to use Trousers in simple Cloudproxy deployments. As a result, this section is informational.

**Clearing and taking ownership of TPM 1.2 with Trousers**

# tpm\_clear --force

Tspi\_TPM\_ClearOwner failed: 0x00000007 - layer=tpm, code=0007 (7), TPM is disabled

We can see that the TPM is disabled, which is why we can’t clear it. This can happen if

we forget to actually enable the TPM in BIOS. The first thing to do would be to actually

enable the TPM in BIOS. But if the TPM has been initialized before, we would receive the

output that can be seen below:

# tpm\_clear --force

TPM Successfully Cleared. You need to reboot to complete this operation. After reboot

the TPM will be in the default state: unowned, disabled and inactive.

This would require us to reboot the computer for changes to take effect. When clearing the

TPM we’ll return it to the default state, which is unowned, disabled and inactive, as

already mentioned. To enable the TPM afterwards, we need the owner password. But since

the TPM owner has been cleared, there is no owner password and we can set a new one

without entering the old one. We can also receive an error like the following:

# tpm\_clear --force

Tspi\_TPM\_ClearOwner failed: 0x0000002d - layer=tpm, code=002d (45), Bad physical presence value

DO NOT SET ANY PASSWORD for the TPM.

# tpm\_takeownership -z -y

If we later want to change either of the commands, we can do it with the tpm\_changeownerauth

command. If we pass the –owner argument to the tpm\_changeownerauth command we’ll be

changing the administration password and if we pass the –srk into the tpm\_changeownerauth

command we’ll be changing the SRK password. We can see the example of both commands in

the output below:

# tpm\_changeownerauth --owner

Enter owner password:

Enter new owner password:

Confirm password:

# tpm\_changeownerauth --srk

Enter owner password:

Enter new SRK password:

Confirm password:

There are 5 keys in TPM:

TPM Endorsement Key (EK): This key is created by the manufacturer and cannot be removed.

Sometimes it can be changed by the owner of the computer.

TPM Storage Key (SRK): Is the 2048 bit RSA key created when configuring the ownership.

This key is stored inside the chip and can be removed. The key is used to encrypt the

Storage Key (SK) and Attestation Identity Key (AIK).# tpm\_setenable --enable

Enter owner password:

Disabled status: false

# tpm\_setactive

Enter owner password:

Persistent Deactivated Status: false

Volatile Deactivated Status: false

There are usually two Endorsement Keys (EK): the public and private one. The private key is always stored at the TPM and cannot even be seen by anyone, while the public key can be displayed with the tpm\_getpubek command.

# tpm\_getpubek

Tspi\_TPM\_GetPubEndorsementKey failed: 0x00000008 - layer=tpm, code=0008 (8), The TPM target command has been disabled

Enter owner password:

Public Endorsement Key:

Version: 01010000

Usage: 0x0002 (Unknown)

Flags: 0x00000000 (!VOLATILE, !MIGRATABLE, !REDIRECTION)

AuthUsage: 0x00 (Never)

Algorithm: 0x00000020 (Unknown)

Encryption Scheme: 0x00000012 (Unknown)

Signature Scheme: 0x00000010 (Unknown)

Public Key:

a350b3a3 3edddc30 06248f4f 5d3eb80a 34fcbea0 83dde002 8dffa703 e116f8b0

eb1962ee a65998b3 384aeb6e 85486be9 0316a6ca a189a5ba 2217b2a2 9da014db

dfbe7731 fb675e7a 438c4775 deea54fb 0c75de5d ba961950 3eda4555 d27a9a30

e94d39d0 a4ea314d a70eaf08 e49dd354 d57ed34d 234220d9 604471a9 86173050

9ff9b0e5 b65cb4b5 5f46a7f9 4378bd7e 8c61b91b ad312974 fef5d70f 84f4484f

e5c95300 0eef76f2 1667443f dc2fa82e 351d945e 6b5f75e8 828d010f 61541552

[...]

## **Troubleshooting TPM 1.2**

**tpm-takeownership fails:** tpm-takeownership assumes the owner of the device is not set. Reset the TPM through BIOS as explained in the main TPM 1.2 section to reset ownership.

**tpm-takeownership not found:** Make sure $GOPATH/bin is in your PATH environment variable.

**Using tpm-clear:** is NOT recommended for resetting the device or clearing ownership, and it is known to leave the TPM in a mucked state from where tpm-takeownership does not work. Reset the TPM through BIOS as explained in the main TPM 1.2 section to reset the device/ownership.

**Tboot Launch Policy for TPM 1.2 (Optional)**

You may build a Launch Control Policy (LCP) which controls what can be booted. If you have no LCP, the default policy will be applied and this should work, so this appendix, like the last is informational only.

Trousers and trousers-devel packages must already be installed in order to build lcptools.

Next you must modify grub so that you can choose the tbooted linux from the boot window.

If the verified launch policy is non-empty, it is extended into PCR 17 by default. Subsequent loaded modules are extended into PCR 18 by default (Check this!). This behavior can be changed with the VLP.

The Grub(2) configuration file is usually in /boot/grub and is called grub.cfg. It is updated automatically when a kernel is updated or when you run update-grub.

Tboot module must be added as the 'kernel' in the grub.conf file.

Note that the Lenovo T410 is known not to work with the Intel IOMMU; it will not successfully boot with TBOOT.

The final grub configuration file will look something like:

menuentry 'Ubuntu Linux 3.0.0-16-generic with TXT' --class ubuntu --class gnu-linux --class gnu --class os {

recordfail

set gfxpayload=text

insmod gzio

insmod part\_msdos

insmod ext2

set root='(hd0,msdos5)'

search --no-floppy --fs-uuid --set=root 8ab78657-8561-4fa8-af57-bff736275cc6

echo 'Multiboot'

multiboot /boot/tboot.gz /boot/tboot.gz logging=vga,memory,serial

echo 'Linux'

module /boot/vmlinuz-3.0.0-16-generic /boot/vmlinuz-3.0.0-16-generic root=UUID=8ab78657-8561-4fa8-af57-bff736275cc6 ro splash vt.handoff=7 intel\_iommu=on

echo 'initrd'

module /boot/initrd.img-3.0.0-16-generic /boot/initrd.img-3.0.0-16-generic

echo 'sinit'

module /boot/sinit51.bin /boot/sinit51.bin

Modify grub.conf to load the policy data file:

Edit grub.conf and add the following:

module /list.data

where you should use the path to this file.

Copy sinit into /boot and change run grub.conf then run update-grub.

Check the /boot directory to make sure tboot.gz is there.

The utility txt-stat in the utils subdirectory of tboot, can be used to view the DRTM boot log.

**Reported problems with TPM 1.2**

The TPM, driver/char/tpm/tpm.c, depends on TPM chip to report timeout values for timeout\_a, b, and d. The Atmel TPM in Dell latitude 6430u, reports wrong timeout values (10 ms each), instead of TCG specified (750ms, 2000ms, 750ms, 750ms for timeout\_a/b/c/d respectively). You can fix the driver code and it will work.

A permissive Tboot policy is required for the non-hypervisor solutions. In this case, the system will boot whatever it finds, but it will still perform measured launch, and clients interacting with the system will still be able to check that the right software was booted by checking the PCRs. Once the hypervisor is written, a more restrictive launch control policy is possible and maybe desirable.

Put 11\_tboot in /etc/grub.d

Information on PCR Usage on TPM 1.2

PCR 17 will be extended with the following values (in this order):

- The values as documented in the MLE Developers Manual

- SHA-1 hash of: tboot policy control value (4 bytes) SHA-1 hash of tboot policy (20 bytes)

: where the hash of the tboot policy will be 0s if TB\_POLCTL\_EXTEND\_PCR17 is clear

PCR 18 It will be extended with the following values (in this order):

- SHA-1 hash of tboot (as calculated by lcp\_mlehash)

- SHA-1 hash of first module in grub.conf (e.g. Xen or Linux kernel)

PCR \* : tboot policy may specify modules' measurements to be extended into PCRs specified in the policy

The default tboot policy will extend, in order, the SHA-1 hashes of all modules (other than 0) into PCR 19.

The LCP consists of policy elements.

To specify launch policy via a list of hashes:

0. sudo bash

1. lcp\_mlehash -c "command line for tboot from grub.cfg" /boot/tboot.gz > mle\_hash

- the command line in this case is the string from /boot/grub/grub.cfg

- after multiboot tboot.gz, e.g., "logging=vga,memory,serial"

- copy and paste:

./lcp\_mlehash -c "logging=vga" /boot/tboot.gz>mle\_hash

2. lcp\_crtpolelt --create --type mle --ctrl 0x00 --minver 17 --out mle.elt mle\_hash

- copy and paste

./lcp\_crtpolelt --create --type mle --ctrl 0x00 --minver 17 --out mle.elt mle\_hash

3. lcp\_crtpollist --create --out list\_unsig.lst mle.elt pconf.elt

- copy and paste

./lcp\_crtpollist --create --out list\_unsig.lst mle.elt pconf.elt

4. lcp\_crtpol2 --create --type list --pol list.pol --data list.data list\_unsig.lst

- copy and paste

./lcp\_crtpol2 --create --type list --pol list.pol --data list.data list\_unsig.lst

5. cp list.pol /boot

- copy and paste

cp owner\_list.data /boot

Next create a verified Launch policy:

1. tb\_polgen/tb\_polgen --create --type nonfatal vl.pol

- copy and paste

../tb\_polgen/tb\_polgen --create --type nonfatal vl.pol

2. tb\_polgen/tb\_polgen --add --num 0 --pcr 18 --hash image

--cmdline "the command line from linux in grub.conf"

--image /boot/vmlinuz-2.6.18.8

vl.pol

- copy and paste

../tb\_polgen/tb\_polgen --add --num 0 --pcr 18 --hash image --cmdline "root=UUID=cf6ae6b5-abb5-4d5d-b823-bd798a0621de ro quiet splash $vt\_handoff" --image /boot/vmlinuz-3.5.0-23-generic vl.pol

3. tb\_polgen/tb\_polgen --add --num 1 --pcr 19 --hash image

--cmdline ""

--image /boot/initrd-2.6.18.8

vl.pol

- copy and paste

../tb\_polgen/tb\_polgen --add --num 1 --pcr 19 --hash image --image /boot/initrd-3.5.0-23-generic vl.pol

If any mle can be launched:

./lcp\_crtpol2 --create --type any --pol any.pol

Define tboot error TPM NV index:

1. lcptools/tpmnv\_defindex -i 0x20000002 -s 8 -pv 0 -rl 0x07 -wl 0x07

-p TPM-password

- copy and paste

../lcptools/tpmnv\_defindex -i 0x20000002 -s 8 -pv 0 -rl 0x07 -wl 0x07

Define LCP and Verified Launch policy indices:

1. lcptools/tpmnv\_defindex -i owner -s 0x36 -p TPM-owner-password

- copy and paste

../lcptools/tpmnv\_defindex -i owner -s 0x36 -p TPM-owner-password

2. lcptools/tpmnv\_defindex -i 0x20000001 -s 256 -pv 0x02 -p TPM-owner-password

- copy and paste

../lcptools/tpmnv\_defindex -i 0x20000001 -s 256 -pv 0x02 -p TPM-owner-password

Write LCP and Verified Launch policies to TPM:

(modprobe tpm\_tis; tcsd;)

1. lcptools/lcp\_writepol -i owner -f [any.pol|list.pol] -p TPM-password

- copy and paste

../lcp\_writepol -i owner -f list.pol -p <ownerauth password>

2. If there is a verified launch policy:

lcptools/lcp\_writepol -i 0x20000001 -f vl.pol -p TPM-password

- copy and paste

../lcptools/lcp\_writepol -i 0x20000001 -f vl.pol -p TPM-password

Use lcp\_crtpollist to sign the list:

1. openssl genrsa -out privkey.pem 2048

2. openssl rsa -pubout -in privkey.pem -out pubkey.pem

3. cp list\_unsig.lst list\_sig.lst

4. lcp\_crtpollist --sign --pub pubkey.pem --priv privkey.pem --out list\_sig.lst

Use openssl to sign the list:

1. openssl rsa -pubout -in privkey.pem -out pubkey.pem

2. cp list\_unsig.lst list\_sig.lst

3. lcp\_crtpollist --sign --pub pubkey.pem --nosig --out list\_sig.lst

4. openssl genrsa -out privkey.pem 2048

5. openssl dgst -sha1 -sign privkey.pem -out list.sig list\_sig.lst

6. lcp\_crtpollist --addsig --sig list.sig --out list\_sig.lst

**TPM 2.0 Installation and Operation**

BIOS, handle limitation,

## **Attest Service**

## **Troubleshooting TPM 2.0**

**Too many open handles:** Run

tpm2\_util.exe –command=Flushall

**TPM2 Error code 0x9a2:**

This error code corresponds to ‘bad authorization’ and is returned when a command has incorrect authorization values. If you encounter this when using CloudProxy, it means your TPM is not provisioned properly, and you would need to clear the TPM.

**TPM2 Error code 0x902:**

This error code is returned when the TPM is out of memory for creating new objects. Run the TPM2\_FlushContext command for all open handles (which can be obtained by running the TPM2\_GetCapability command).

**TPM2\_Clear on the Intel NUC 5i5MYHE:**

Clearing the TPM has the effect of setting all authorization values to *emptyAuth* (i.e. empty string as password). Clearing a TPM can be done through the maintenance screen of the BIOS, which is accessed by booting up the machine with the yellow BIOS jumper removed, and pressing the Esc key when the startup BIOS screen is shown.

**Tboot**

To build tboot you first need to install trousers and libtspi-dev.

Installing TBOOT

1. Download the source tarball from <https://sourceforge.net/projects/tboot/>
2. In the untarred source directory run:  
   make
3. In the same directory as above, run  
   sudo make install
4. Check the /boot directory contains the tboot.gz file
5. Download the SINIT AC module corresponding to your processor from  
   <https://software.intel.com/en-us/articles/intel-trusted-execution-technology>
6. Copy the SINIT \*.BIN file to your /boot directory
7. To start using tboot, you need to update your bootloader configuration. If using grub2, run  
   sudo update-grub  
   And check that /boot/grub/grub.cfg now contains an entry for tboot which looks like:

menuentry 'Ubuntu GNU/Linux, with tboot 1.9.4 and Linux 4.4.0-24-generic' --class ubuntu --class gnu-linux --class gnu --class os --class tboot {

insmod multiboot2

insmod part\_gpt

insmod ext2

set root='hd0,gpt2'

if [ x$feature\_platform\_search\_hint = xy ]; then

search --no-floppy --fs-uuid --set=root --hint-bios=hd0,gpt2 --hint-efi=hd0,gpt2 --hint-baremetal=ahci0,gpt2 1df958d9-c01d-43d8-a1b2-18d022843d3f

else

search --no-floppy --fs-uuid --set=root 1df958d9-c01d-43d8-a1b2-18d022843d3f

fi

echo 'Loading tboot 1.9.4 ...'

multiboot2 /boot/tboot.gz logging=serial,memory

echo 'Loading Linux 4.4.0-24-generic ...'

module2 /boot/vmlinuz-4.4.0-24-generic root=UUID=1df958d9-c01d-43d8-a1b2-18d022843d3f ro quiet splash intel\_iommu=on noefi

echo 'Loading initial ramdisk ...'

module2 /boot/initrd.img-4.4.0-24-generic

echo 'Loading sinit 5th\_gen\_i5\_i7\_SINIT\_79.BIN ...'

module2 /boot/5th\_gen\_i5\_i7\_SINIT\_79.BIN

}

1. If using tboot with cloudproxy, you need to adjust your bootloader configuration differently (to add the initramfs). Instructions to do so can be found in a subsequent appendix.

More information about Tboot can be found in the README in the Tboot source directory.

Tboot will copy and alter the e820 table provided by GRUB to "reserve" its own memory plus the TXT memory regions. These are marked as E820\_UNUSABLE or E820\_RESERVED so that the patched Xen code can prevent them from being assigned to dom0. The e820 table is not altered if the measured launch fails for any reason.

**Initramfs**

Yours initramfs must contain the Cloudproxy root software and any shared libraries required by the kernel and the programs it starts with root privilege. We describe below how to do this.

For other (stacked) Cloudproxy hosts or applications, you have three choices:

1. Ensure all all programs are “statically linked” so you do not rely on “untrusted” libraries.
2. Ensure that only libraries in intiramfs are dynamically loaded with your application.
3. Control library loading from within your Cloudproxy application and make sure you load the library into memory and check it hash against a policy signed statement before linking to it.

Decompress and unpack the existing initramfs

cd /tmp

mkdir init

cd init

cp /boot/initramfs.img-`uname -r` initrd.gz

gunzip -c -9 initrd.gz | cpio -i -d -H newc --no-absolute-filenames

Copy the dynamic link libraries for the executables into the filesystem to the resulting directory.

Copy the runtime directory into the filesystem, and get ifconfig, too

mkdir -p home/jlm/jlmcrypt

cp -r /home/jlm/jlmcrypt/\* home/jlm/jlmcrypt/

cp /sbin/ifconfig sbin/ifconfig

Change the initscript (init) to run dmcrypt and change the way the

system disk is mounted.

vim init

Here is a simple script that works:

-- start simple script

#!/bin/sh

[ -d /dev ] || mkdir -m 0755 /dev

[ -d /root ] || mkdir -m 0700 /root

[ -d /sys ] || mkdir /sys

[ -d /proc ] || mkdir /proc

[ -d /tmp ] || mkdir /tmp

mkdir -p /var/lock

mount -t sysfs -o nodev,noexec,nosuid sysfs /sys

mount -t proc -o nodev,noexec,nosuid proc /proc

# Some things don't work properly without /etc/mtab.

ln -sf /proc/mounts /etc/mtab

grep -q '\<quiet\>' /proc/cmdline || echo "Loading, please wait..."

# Note that this only becomes /dev on the real filesystem if udev's scripts

# are used; which they will be, but it's worth pointing out

if ! mount -t devtmpfs -o mode=0755 udev /dev; then

echo "W: devtmpfs not available, falling back to tmpfs for /dev"

mount -t tmpfs -o mode=0755 udev /dev

[ -e /dev/console ] || mknod -m 0600 /dev/console c 5 1

[ -e /dev/null ] || mknod /dev/null c 1 3

fi

mkdir /dev/pts

mount -t devpts -o noexec,nosuid,gid=5,mode=0620 devpts /dev/pts || true

mount -t tmpfs -o "nosuid,size=20%,mode=0755" tmpfs /run

mkdir /run/initramfs

# compatibility symlink for the pre-oneiric locations

ln -s /run/initramfs /dev/.initramfs

/sbin/ifconfig lo 127.0.0.1

# can set up other networks here as needed, e.g., on eth0

# mount /boot as a place to put keys between reboots (e.g., for tcService.exe)

mkdir /boot

mount /dev/sda1 /boot

/bin/busybox sh

-- end simple script

- untested:

swapoff -a

cryptsetup [-c aes -h sha256] -s 128 -d /dev/urandom create swap /dev/sda1

mkswap /dev/mapper/swap

swapon /dev/mapper/swap

Put initramfs back together

find . | cpio -H newc -o|gzip -9 > ../initrd.img-new

Copy it to the boot directory

sudo cp initrd.gz /boot/initrd.img-staticLinux

Change /etc/grub.d to use this new initramfs.

To configure Linux to boot by mounting an initramfs image internally, set the

following items on the kernel config:

CONFIG\_BLK\_DEV\_INITRD=y

CONFIG\_INITRAMFS\_SOURCE=<Initramfs cpio image path>

After making these changes to the settings, re-compile the kernel. Finally, the kernel

can be booted as follows (for instance, we report a boot on a mb442 by using a "vmlinux" with the above settings enabled):

host% st40load\_gdb -t stmc:mb442:st40 -c sh4tp -b vmlinux mem=64m

No other parameters have to be passed to st40load\_gdb to boot with initramfs, as the

kernel mounts that image automatically.

To boot Linux by using the initramfs image, create a typical ext2 (or ext3) filesystem

structure in which the only difference with respect to the standard ext2/3 root filesystem

used in SysV, or busybox, is related to the init file.

Usually, the init file is placed under /sbin (for both SysV and Busybox). In the initramfs

rootfs image, the init file has to be placed under the root, /, as the kernel tries to

execute /init instead of /sbin/init in case the initramfs image was mounted after boot.

A typical initramfs filesystem structure is as follows:

target% ls

bin dev etc home include init lib mnt proc sys sbin tmp usr var

The tool mkshinitramfs has been created to improve the process of initramfs rootfs

image creation. The current version of the tool is 1.0. To get information about the

tool's parameters, type the following command line:

host# ./mkshinitramfs -h

mkshinitramfs-1.0,

usage: mkshinitramfs [-h|-H Help]

mkshinitramfs [-o|O: <Initramfs CPIO image with switch option to HDD(/dev/sda1)>]

mkshinitramfs [-s|S: <Initramfs CPIO image with shell on Initramfs>]

mkshinitramfs [-p|P: <target rootfs path> | default: /opt/STM/STLinux-2.3/devkit/sh4/target/]

mkshinitramfs [-k|K: <SH kernel version> | default: 2.6.23\_stm23\_0121]

mkshinitramfs [-b|B: <used board> | default: mb442 (STi710x based board)]

mkshinitramfs must be executed as "root" on the host machine in which a full target root

filesystem has previously been installed. It is configured to use default parameters,

as listed in the output from the -h option. To change any of the parameters, apply the

command line options listed in the help.

The tool mkshinitramfs creates a short initramfs. If invoked with the -s option, the

generated initramfs is the final rootfs. If invoked with the -o option, the generated

initramfs is a temporary rootfs to be switched to the real one on the HDD.

The script mkshinitramfs internally defines some variables that are useful when defining

which files, libraries, scripts and tools are to be placed on the initramfs image.

The variables are:

$DIRS

$BINFILES

$SBINFILES

$ETCFILES1

$USRBINFILES

Version 1.0 of the mkshinitramfs tool can be downloaded from mkshinitramfs tool as a

compressed tar.gz file.

If the initramfs rootfs is created to be used temporarily before switching to the real

target rootfs on a hard disk drive, a setup script is needed, which is then passed to

the chroot in order to setup the final real rootfs properly. This script loads the user

space services needed at runtime, such as klogd, udev, D-Bus, and so forth.

If the -o option is used, mkshinitramfs generates a CPIO image in which the following

command line is inserted after the kernel mounts the initramfs:

mount /dev/sda1 /mnt

chroot /mnt /etc/init.d/rcS-initramfs

**Dmcrypt**

Dmcrypt is a standard Linux component, we use it to encrypt page tables so that there is no sensitive information on disks. As a result, while the system paging disk should be in the “cage” during operation, these disks do not contain sensitive information and do not have to be specially handled after operation. Disks do not have to be wiped.

fdisk to make partitions (/dev/sda)

mkfs.ext2 to make file system

change to single user mode

grub-install root-directory=/dev/sda

CRYPTDISKS\_ENABLE=Yes in /etc/defaults/cryptdisks

/etc/crypttab

swap /dev/hda1 /dev/urandom swap

/etc/fstab

/dev/swapper/swap none

swap sw,pri=1 0 0

For swap:

swapoff -a

cryptsetup [-c aes -h sha256] -s 128 -d /dev/urandom create swap /dev/sda1

mkswap /dev/mapper/swap

swapon /dev/mapper/swap

Shell script prototype

#

# For debian, first do the following:

#

# Change to single user mode

# cat /proc/swaps (to find out swap device)

# /sbin/runlevel (to find runlevel)

# /sbin/telinit 1 (to go single user)

# ctrl-alt-f7 puts Linux into console mode.

#

# /etc/defaults/cryptdisks

# CRYPTDISKS\_ENABLE=Yes

# /etc/crypttab

# swap /dev/sda5 /dev/urandom swap

# /etc/fstab

# /dev/mapper/swap none

# swap sw,pri=1 0 0

# /etc/crypttab

# swap /dev/sda5 /dev/urandom cipher=aes-cbc-essiv:sha256,size=256,hash=sha256,swap

# /etc/fstab

# /dev/mapper/cryptoswap none swap sw 0 0

#

# /dev/sda5 is swap device

#

# Ref: The whole disk Nov, 2006, Linux-magazine.com, Michael Nerb

#

swapoff -a

cryptsetup -c aes -h sha256 -s 128 -d /dev/urandom create swap /dev/sda5

mkswap /dev/mapper/swap

swapon /dev/mapper/swap

#

# To remove:

# swapoff /dev/mapper/swap

# cryptsetup [luks] remove swap

**Grubby, Grub, Grub (Optional)**

This appendix is informational, tboot does all of this automatically in the normal course of events.

The new tboot module must be added as the 'kernel' in the grub.conf file. The existing 'kernel' entry should follow as a 'module'. The SINIT ACM module must be added to the grub.conf boot config as the last module, for example:

root (hd0,1)

kernel /tboot.gz logging=serial,vga,memory

module /vmlinuz-2.6.18 root=/dev/VolGroup00/LogVol00 ro

module /initrd-2.6.18.img

module /Q35\_SINIT\_17.BIN

The kernel module is tboot. The next is the Linux (possibly KVM enabled) kernel. Next is the initramfs and finally the ACM module.

GRUB2 does not pass the file name in the command line field of the multiboot entry (module\_t::string). Since the tboot code is expecting the file name as the first part of the string, it tries to remove it to determine the command line arguments, which will cause a verification error. The "official" workaround for kernels/etc. that depend on the file name is to duplicate the file name in the grub.config file like below:

menuentry 'Xen w/ Intel(R) Trusted Execution Technology' {

recordfail

insmod part\_msdos

insmod ext2

set root='(/dev/sda,msdos5)'

search --no-floppy --fs-uuid --set=root 4efb64c6-7e11-482e-8bab-07034a52de39

multiboot /tboot.gz /tboot.gz logging=vga,memory,serial

module /xen.gz /xen.gz iommu=required dom0\_mem=524288 com1=115200,8n1

module /vmlinuz-2.6.18-xen /vmlinuz-2.6.18-xen root=/dev/VolGroup...

module /initrd-2.6.18-xen.img /initrd-2.6.18-xen.img

module /Q35\_SINIT\_17.BIN

}

## **Setting up a Cloudproxy enabled KVM host**

In this section we will see how to set up a Cloudproxy enabled KVM host, which can launch independent Cloudproxy VMs (i.e. VMs with a stacked Cloudproxy host running)

**Step 1: Run a SoftTao hosted KVM**

This is really just about running KVM. The root Tao of our CloudProxy KVM host will be a “soft” Tao: i.e. a dummy Tao based on a keyset that is stored on disk, encrypted and integrity protected by a password.

The guest VMs will be CoreOS instances.

1. **Generate soft Tao.**We set up the Tao domain directory and the host directory, where the domain and host configuration information will be stored. We copy in a domain template which we will use in this example and setup the soft Tao which generates a password protected keyset in the linux\_tao\_host directory.  
     
   mkdir /tmp/domain  
   cd /tmp/domain  
   mkdir linux\_tao\_host  
   cp $GOPATH/src/github.com/jlmucb/\  
    cloudproxy/go/apps/simpleexample/SimpleDomain/\  
    domain\_template.simpleexample .  
   tao domain newsoft \  
    -config\_template domain\_template.simpleexample \  
    -soft\_pass xxx ./linux\_tao\_host
2. **Initialize domain**We initialize the domain which will create policy keys, saved in the domain directory and protected by the password. It will also create a tao.config file which stores all the domain configuration information and is used by the host to load the domain.

tao domain init \  
 -tao\_domain . \  
 -config\_template domain\_template.simpleexample \  
 -pass xxx

1. **Create linux\_host image**We statically build a linux host image (so that it is executable in the VM) and create a tarball of the linux\_host binary and the host/domain configuration information it needs to run. When launching a VM, the KVM Cloudproxy unpacks this, mounts it on the VM and runs linux\_host as a stacked Cloudproxy host.CGO\_ENABLED=0 go install -a \  
    -installsuffix nocgo \  
    github.com/jlmucb/cloudproxy/go/apps/linux\_host  
   cp $GOPATH/bin/linux\_host .  
   tar -C . -czf linux\_host.img.tgz $(ls .)
2. **Get CoreOS image**Get the latest stable image of CoreOS.curl -G http://stable.release.core-os.net/amd64-usr/\  
    current/coreos\_production\_qemu\_image.img.bz2 > \  
    coreos\_production\_qemu\_image.img.bz2  
   bunzip2 coreos\_production\_qemu\_image.img.bz2
3. **Setup ssh-agent**We generate a key pair and setup ssh-agent for SSHing into the VM instance.  
     
   ssh-keygen -t rsa -f ./id\_rsa  
   ssh-add id\_rsa
4. **Initialize and start host**We initialize and start the KVM Cloudproxy hosttao host init \  
    -root \  
    -tao\_domain . \  
    -pass xxx \  
    -hosting kvm\_coreos \  
    -kvm\_coreos\_img coreos\_production\_qemu\_image.img \  
    -kvm\_coreos\_ssh\_auth\_keys id\_rsa.pub  
     
   tao host start \  
    - tao\_domain . \  
    - host ./linux\_tao\_host
5. **Launch hosted program (i.e. VM)**  
   We launch a Cloudproxy VM through the Cloudproxy KVM host. We create another temporary directory where the linux\_host tarball is unpacked and mounted on the VM and run from.  
     
   mkdir another\_tmp  
   tao\_launch run \  
    -tao\_domain . \  
    -host ./linux\_tao\_host \  
    -verbose kvm\_coreos:linux\_host.img.tgz \  
    -- linux\_host.img.tgz another\_tmp 2222

**Step 2: A custom KVM Host**

Here is a quick description of how to build the kernel for host and guest.

variables: $KERNEL is the kernel source directory (e.g., /usr/src/linux-3.11.0), $CODE is the Cloudproxy directory

export KERNEL="/usr/src/linux-lts-quantal-3.5.0"

- Make sure you have all the prerequisites for building the kernel

- get the kernel source and make its root directory be $KERNEL

- navigate to ${CODE}/kvm/host-kernel

- execute the commands

- ./apply-patches.sh $KERNEL

- ./copy\_to\_kernel.sh $KERNEL

make menuconfig

disable loadable module support

edit config CONFIG\_ACPI=n

The apply-patches.sh command might fail, depending on the vintage of the kernel you have. If the patches fail, they are fairly easy to fix by hand. You can look at the patches to see what they do:

- the Makefile in ${KERNEL}/drivers/misc needs to have three extra lines, one obj-y += DIR for each of the three directories we added (\*tcio\*)

- the Makefile in ${KERNEL}/arch/x86/kvm needs to add vmdd.o to the dependencies of kvm.o

- ${KERNEL}/arch/x86/kvm/x86.c needs to have the lines added from the patch in ${CODE}/kvm/host-kernel/arch/x86/kvm/x86.c.patch (just acouple of lines)

- copy a working config over to $KERNEL as .config. This is more important than it may seem at first glance. Often dependencies in make menuconfig make getting an appropriate configuration (e.g.-one that CONFIG\_INTEL\_TXT=y) difficult. A sample .config file (for Linux 3.5.7) is in config.sample in this directory. NOTE: If you're building in the VM make sure you copy a .config from a working VM kernel.

- run

- yes "" | make oldconfig

- yes "" | make localmodconfig

- make (with a -j factor appropriate for your machine)

- sudo make modules\_install

- sudo make install

- and you should have a copy of the new kernel in /boot, ready to go.

- update the tboot script for this kernel and try to tboot it.

**Step 3: Building and running VMs with libvirt**

Make sure your VM has at least 20MB of disk

1. Install via virt-manager a fresh VM from a CD.

2. SSH the jlmcrypt directory into the VM.

apt-get install openssh-server

sudo service ssh start

sudo stop ssh

sudo start ssh

sudo restart ssh

sudo status ssh

ssh jlm@192.168.122.244

sftp

put jlmcrypt.tar .

3. Save the VM Image in virtmanager. You can find the IP address to SSH to by going into the VM and typing ifconfig -a.

4. Save the original libvirt xml to a safe place. For example,

virsh dumpxml KvmTestGuest > /home/jlm/jlmcrypt/vms/KvmTestGuestImage.xml

5. Copy the kernel-image file and initramfs file for the CloudProxy partition to the place you want to save them. In this example, I use /home/jlm/jlmcrypt/vms/kernel and /home/jlm/jlmcrypt/vms/initram.

6. Change the boot options for your vm (in virt-manager, for example) so that it does the direct kernel/initram boot using the files named in step 6.

7. Save the new libvirt xml to a safe place. For example,

virsh dumpxml KvmTestGuest > /home/jlm/jlmcrypt/vms/KvmTestGuestBoot.xml.

8. Copy the direct boot xml into a template file that you will reference

when you tcLaunch the VM. For example, cp /home/jlm/jlmcrypt/vms/KvmTestGuestBoot.xml /home/jlm/jlmcrypt/vms/KvmTestGuestTemplate.xml

9.Edit the template file.

Replace the value of the name tag (which should have the name of

vm originally) with %s. For example,

<name>%s</name>

Replace the kernel and image tag values with %s, getting

<kernel>%s</kernel>

<initrd>%s</initrd>

Replace the disk source file value with %s, getting:

<disk type='file' device='disk'>

<driver name='qemu' type='raw'/>

<source file='%s'/>

<target dev='hda' bus='ide'/>

<address type='drive' controller='0' bus='0' unit='0'/>

</disk>

**Running the newly-installed guest**

sudo /usr/local/kvm/bin/qemu-system-x86\_64 vdisk.img -m 384

Download and install KVM: You can use the package included in Ubuntu 7.10, just execute: apt-get install kvm You can also download the last release of KVM and compile it.

You also need the linux-headers packages for the Kernel you are using.

First of all, we need the KVM package. You can find the actual release at http://sourceforge.net/projects/kvm/. Download it to your server:

wget link/to/file /usr/src/

Now unpack the content.

cd /usr/src/

tar -xzf file.tar.gz

cd folder/to/kvm

Before compiling KVM make sure that your CPU supports virtualization and if that option is activated in the BIOS. Compile KVM.

./configure

make

make install

Now load the KVM modules:

If you have an Intel CPU load:

modprobe kvm

modprobe kvm\_intel

If you have an AMD CPU load:

modprobe kvm

modprobe kvm\_amd

Creating the network bridge First, install bridge-utils: apt-get install bridge-utils

If you want to connect to your virtual machine later, you need to set up a network bridge. Edit /etc/network/interfaces like this (make sure to insert your public IP Address):

auto lo

iface lo inet loopback

auto br0

iface br0 inet static

address xxx.xxx.xxx.xxx

netmask xxx.xxx.xxx.xxx

gateway xxx.xxx.xxx.xxx

bridge\_ports eth0

bridge\_stp off

bridge\_maxwait 5

Also edit /etc/qemu-ifup like this:

#!/bin/sh

/sbin/ifconfig $1 0.0.0.0 promisc up

/usr/sbin/brctl addif br0 $1

sleep 2

I recommend restarting your server at this point. If you are able to reconnect, your bridge is working.

Creating a virtual disk for a virtual machine & install a system into it. Create an .img file for installation. This file acts as a virtual disk for your vm.

**Host Certificates**

Put some example policy and cert certificates here.

**SimpleExample with a TPM 1.2 Tao**

**SimpleExample with a TPM 2.0 Tao**

**Preparing the environment**

Generate and sign the endorsement cert with the Policy Key.

**The attest quote service**

Unlike TPM 2.0, the key signing the TPM2 Tao attest is a generated signing key called the quote key. It is generated by TPM2Tao when it is first run. The quote key, after it is generated, must obtain a policy key signed certificate. This signing operation is done by the Quote attest service. The quote attest service employs the MakeCredential/ActivateCredential facilities of TPM2.0 in conjunction with the endorsement cert.

The protocol operates as follows:

1. TPM2Tao generates a quote key uses the Quote key to attest to itself. It der serializes the Quote key and transmits the quote, taoname, endorsement certificate and the serialized quote key to the Attest service.
2. The attest service validates the quote, and signs a certificate naming the quote key and its Tao Principal Name. This certificate is encrypted using the MakeCredential algorithm specified in TPM2. This algorithm uses the endorsement key and properties of the quote key (likes its TPM2.0 name) so that the encrypted certificate can only be decrypted on the TPM with the active quote key and and active endorsement key corresponding to the endorsement certificate. It returns the encrypted certificate and associated information to TPM2Tao.
3. TPM2Tao uses the ActivateCredential algorithm operating inside the TPM to decrypt the certificate. The Tao uses this certificate to authenticate the Quote key in the same manner that TPMTao uses the AIK.

Run the attest quote service

**SimpleExample in VM using stacked host, KVM host undert TPM 2.0 Tao**

1. John isat [manferdelli@google.com](mailto:manferdelli@google.com) or [jlmucbmath@gmail.com](mailto:jlmucbmath@gmail.com); Sid is at [sidtelang@google.com](mailto:sidtelang@google.com). Cloudproxy is based on work with Tom Roeder ([tmroeder@google.com](mailto:tmroeder@google.com)), Fred Schneider (Cornell) and Kevin Walsh ([kevin.walsh@holycross.edu](mailto:kevin.walsh@holycross.edu) ). [↑](#footnote-ref-1)
2. A subtle point: Dmcrypt at the time of this writing, encrypts but does not provide integrity protection. As a result, the “paging disk” (which might be flash or spinning media) should be in the “physical protection barrier” described in the Security Considerations section of this document. [↑](#footnote-ref-2)